SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( TRIN5127UP_MT
 comment ( release 1, shape and original textures by Hauke Hey,© June 2010 )
 comment( Trinity Covered Hopper 5127 cuft, UP logo )
 Type ( Freight )
 Name ( "UP 5127 cf cov. hop. empty" )
 WagonShape ( TRIN5127UP.s )
 Size ( 3.23m 4.65m 18.3m )
 Mass ( 30t )
 WheelRadius ( 36in/2 )
 InertiaTensor ( Box (3.23m 4.65m 18.3m) )
 Coupling (
  Type ( Automatic )
  Spring (
   Stiffness ( 1e6N/m 5e6N/m )
   Damping ( 1e7N/m/s 1e8N/m/s )
   Break ( 2e7N 2e7N )
   r0 ( 2cm 4cm )
  )
  Velocity ( 0.1m/s )
 )
 Adheasion ( 0.2 0.4 2 0 )
 DerailRailHeight ( 4cm )
 DerailRailForce ( 2.5*120t )
 DerailBufferForce ( 400kN )
 NumWheels ( 4 )
 Friction (
  1080N/m/s  -0.05  1.3mph  3.98N/m/s  1.78
  5.1N/rad/s  1  -1rad/s  0  1
 )

 Lights ( 2
    
   Light (
   comment( Rear red light, dim )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 2
    State (
     Duration ( 0.3 )
     LightColour ( 80ff0000 )
     Position ( 0.3 0.9 -9.4 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 0.5 )
    )    
    State (
     Duration ( 0.7 )
     LightColour ( 00000000 )
     Position ( 0.3 0.9 -9.4 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
   )
  )
  Light (
   comment( Rear red light, bright )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 2
    State (
     Duration ( 0.3 )
     LightColour ( 80ff0000 )
     Position ( 0.3 0.9 -9.4 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 0.5 )
    )    
    State (
     Duration ( 0.7 )
     LightColour ( 00000000 )
     Position ( 0.3 0.9 -9.4 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
   )
  )
 )

 BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
 BrakeSystemType( "Air_single_pipe" )
 MaxBrakeForce( 40kN )

 MaxHandbrakeForce( 35kN )
 NumberOfHandbrakeLeverSteps( 100 )

 TripleValveRatio( 2.5 )
 MaxReleaseRate( 2.3 )
 MaxApplicationRate( 1.7 )
 MaxAuxilaryChargingRate( 1 )
 EmergencyResCapacity( 2.6 )
 EmergencyResChargingRate( 1 )
 EmergencyBrakeResMaxPressure( 90 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 64 )

   Sound ( "GenFreightWag1.sms" )
)